 **BRANDON CLASPILL – PT RESPONSE ANSWERS INCLUDED**

**Packet Tracer - Examine the ARP Table**

# Addressing Table

|  |  |  |  |
| --- | --- | --- | --- |
| **Device** | **Interface** | **MAC Address** | **Switch Interface** |
| Router0  *Router0* | Gg0/0 | 0001.6458.2501 | G0/1 |
| S0/0/0 | N/A | N/A |
| Router1  *Router1* | G0/0 | 00E0.F7B1.8901 | G0/1 |
| S0/0/0 | N/A | N/A |
| 10.10.10.2 | Wireless | 0060.2F84.4AB6 | F0/2 |
| 10.10.10.3 | Wireless | 0060.4706.572B | F0/2 |
| 172.16.31.2 | F0 | 000C.85CC.1DA7 | F0/1 |
| 172.16.31.3 | F0 | 0060.7036.2849 | F0/2 |
| 172.16.31.4 | G0 | 0002.1640.8D75 | F0/3 |

# Instructions Part 1: Examine an ARP Request

**Step 1: Generate ARP requests by pinging 172.16.31.3 from 172.16.31.2.**

*Open a command prompt*

1. Click **172.16.31.2** and open the **Command Prompt**.
2. Enter the **arp -d** command to clear the ARP table.

*Close a command prompt*

1. Enter **Simulation** mode and enter the command **ping 172.16.31.3**. Two PDUs will be generated. The **ping** command cannot complete the ICMP packet without knowing the MAC address of the destination. So the computer sends an ARP broadcast frame to find the MAC address of the destination.
2. Click **Capture/Forward** once. The ARP PDU moves **Switch1** while the ICMP PDU disappears, waiting for the ARP reply. Open the PDU and record the destination MAC address.

Question:

Is this address listed in the table above? **NO *Type your answers here.***

**Packet Tracer - Examine the ARP Table**

1. Click **Capture/Forward** to move the PDU to the next device.

Question:

How many copies of the PDU did **Switch1** make? **3**

***Type your answers here.***

What is the IP address of the device that accepted the PDU? **IP Address - 172.16.31.3**

***Type your answers here.***

1. Open the PDU and examine Layer 2.

Question:

What happened to the source and destination MAC addresses?

* **Source MAC Address became Destination MAC Address.**
* **FFFF:FFFF:FFFF Converted to MAC address of 172.16.31.3**

***Type your answers here.***

1. Click **Capture/Forward** until the PDU returns to **172.16.31.2**.

Question:

How many copies of the PDU did the switch make during the ARP reply?

**The Switch made One Copy of the PDU during ARP reply.**

***Type your answers here.***

**Step 2: Examine the ARP table.**

1. Note that the ICMP packet reappears. Open the PDU and examine the MAC addresses.

Question:

Do the MAC addresses of the source and destination align with their IP addresses? **YES**

***Type your answers here.***

1. Switch back to **Realtime** and the ping completes.
2. Click **172.16.31.2** and enter the **arp –a** command.

Question:

To what IP address does the MAC address entry correspond? **IP Address – 172.16.31.3**

***Type your answers here.***

In general, when does an end device issue an ARP request?

**When the receiver’s MAC Address in Unknown.**

***Type your answers here.***

# Part 2: Examine a Switch MAC Address Table

**Step 1: Generate additional traffic to populate the switch MAC address table.**

*Open a command prompt*

1. From **172.16.31.2**, enter the ping **172.16.31.4** command.
2. Click **10.10.10.**2 and open the **Command Prompt**.
3. Enter the **ping 10.10.10.3** command.

Question:

How many replies were sent and received? **4 Replied Sent, 4 Received.**

***Type your answers here.***

*Close a command prompt*

**Step 2: Examine the MAC address table on the switches.**

1. Click **Switch1**and then the **CLI** tab. Enter the **show mac-address-table** command.

Question:

Do the entries correspond to those in the table above? **YES**

***Type your answers here.***

1. Click **Switch0**, then the **CLI** tab. Enter the **show mac-address-table** command.

Questions:

Do the entries correspond to those in the table above? **YES**

**Packet Tracer - Examine the ARP Table**

***Type your answers here.***

Why are two MAC addresses associated with one port?

**They both are connected to the one port which is through the Access Point.**

***Type your answers here.***

# Part 3: Examine the ARP Process in Remote Communications

**Step 1: Generate traffic to produce ARP traffic.**

*Open a command prompt*

1. Click **172.16.31.2** and open the **Command Prompt**.
2. Enter the **ping 10.10.10.1** command.
3. Type **arp –a**.

Question:

What is the IP address of the new ARP table entry? **IP Address – 172.16.31.1**

***Type your answers here.***

1. Enter **arp -d** to clear the ARP table and switch to **Simulation** mode.
2. Repeat the ping to 10.10.10.1.

Question:

How many PDUs appear**?**

**2 PDU’s Appear**.

***Type your answers here.***

*Close a command prompt*

1. Click **Capture/Forward**. Click the PDU that is now at **Switch1**.

Question:

What is the target destination IP destination address of the ARP request? **IP Address – 172.16.31.1**

***Type your answers here.***

1. The destination IP address is not 10.10.10.1.

Question:

Why? **This is because the gateway address of the router interface is stored in the IPv4 configuration of the hosts. If the receiving host is not on the same network, the source uses the ARP process to determine a MAC address for the router interface serving as the gateway.**

***Type your answers here.***

**Step 2: Examine the ARP table on Router1.**

1. Switch to **Realtime** mode. Click **Router1** and then the **CLI** tab.
2. Enter privileged EXEC mode and then the **show mac-address-table** command.

Question:

How many MAC addresses are in the table? Why?

**There aren’t any MAC Addresses shown because this command doesn’t have the same meaning on the router as it does for the switch.**

***Type your answers here.***

1. Enter the **show arp** command.

Questions:

Is there an entry for **172.16.31.2**? **YES**

***Type your answers here.***

What happens to the first ping in a situation where the router responds to the ARP request?

**The first ping will typically time out in this situation.**

***Type your answers here.***

*End of document*